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CITX 1151: Understanding TCP/IP


Class A, B or C?





Loopback address?





Network address?





Valid host IP address





Invalid host IP address





Broadcast address?





Checking validity of a host IP address





Decision criteria:


Addresses 1.x.x.x to 223.x.x.x





Decision criteria:


Address 127.x.x.x





Decision criteria:


Host bits all 0’s





Decision criteria:


Host bits all 1’s
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